* A study to compare total and polarized radiance measurements effect on aerosol retrievals is presented.
* No clear advantage to using the linearly polarized measurement for aerosol retrievals.
* Only disadvantage is the lower signal levels from measuring a polarized radiance.
* Between polarizations no significant change in the observed bias is observed.
* Linearly-polarized measurement can be used to achieve approximately equal results.